Wit-E-Board

# Technical Challenges

## Accuracy

Location must be determined within 3mm

### Ultrasonic BFSK + Phase Shift Method

## Synchronization

## Tilt Compensation

Tilt must be determined within \_?\_ degrees

### Gyroscope

## Data Transmission

## Multi-Beacon Support

Multiple markers must be able to be used at once

### CDMA?